LWL frame set for 2 x E2000®, SC-Simplex, LC-Duplex, RAL9010

LWL frame set for 2 x E2000®, SC-Simplex, LC-Duplex, RAL9010,

unloaded frame set for 2 feed-through couplings. The set offers 2 ports for E2000® Simplex, SC Simplex or LC Duplex and a 40° outlet. The outer ring measures 80x80mm and the central disc 50x50mm according to DIN49075. With the adapter plate of the switch program manufacturer, the set is compatible with any switch program. An inscription field is integrated.

The scope of delivery includes: 1 x metal frame, 1 x outer ring, 1 x central disc, 4 x M2 screws.

Surface-mounted: Yes

Flush-mounted: Yes

Sewer installation: Yes

Floor tank/underfloor installation: Yes

Mounting type: Screw

With socket/coupling: No

Max. Equipment (adapter): 2

Suitable for coupling: SC Simplex/LC Duplex/E2000®

With text field: Yes

Central plate: Yes

Central plate according to: DIN 49075

Cover frame: Yes

Outlet direction: angled

Dust protection: without

Support ring material: zinc die casting

Material central plate: ABS plastic

Colour: white

RAL number: 9010

Dimensions: 80mm x 80mm

Make: EFB-Elektronik GmbH

Item no.: ET-25085FO