FTTH IP65 connection box 2 ports

FTTH IP65 connection box 2 ports,

unassembled 2-port connection box made of plastic suitable for SC-Simplex/ LC-Duplex/ E2000® couplings, which has an overlength fibre holder. In addition to a swivelling splice cassette, the connection box contains a cable sheathing.

The FTTH IP65 connection box is used in optical telecommunication networks, LAN, CATV networks, FTTH networks as well as PON and G-PON.

Supplied with 2x shrink splice protection and material for wall mounting.

Field of application: Exterior

Mounting type: Wall mounting

Possibility of mast mounting: No

Material: plastic

Colour: White

Number of cable entries: 3 (1x max. 10mm / 2x max. 4mm)

Maximum number of fibres: 2

splice protection type: shrink / crimp

Coupling type: SC Simplex/LC Duplex/E2000®

Max. Equipment (adapter): 2

IP Protection class IP65

Protection against foreign bodies and contact: Protection against dust ingress

Water protection: Protection against water jets

Dimensions: hxbxt 165mm x 100mm x 30mm

Temperature range: -25°C - 70°C

Access protection: Special screw

Make: EFB-Elektronik GmbH

Item no.: FTTH-BOX-OUT-4