FTTH indoor connection box for 4 fibres, 4 couplings

FTTH Indoor connection box for 4 fibres, 4 couplings,

unloaded 4-ports connection box made of plastic suitable for SC-Simplex/ LC-Duplex/ E2000® couplings, which has a fibre overlength holder and a swivelling splice cassette. The FTTH indoor connection box is used in optical telecommunication networks, LAN, CATV networks, FTTH networks as well as PON and G-PON.

Supplied with 4x shrink splice protection and material for wall mounting. When using crimp splice protection, please note that it cannot be permanently inserted.

Field of application: Inside

Mounting type: Wall mounting

Possibility of mast mounting: No

Material: plastic

Colour: White

Maximum number of fibres: 4

Splice protection type: Shrink / Crimp

Coupling type: SC Simplex/LC Duplex/E2000®

Max. Equipment (adapter): 4

IP Protection class IP20

Protection against foreign bodies and accidental contact: Protection against medium-sized foreign bodies

Water protection: No protection

Dimensions: hxbxt 150mm x 110mm x 34mm

Temperature range: 0°C - 50°C

Access protection: Without

Make: EFB-Elektronik GmbH

Item no.: FTTH-BOX-IN-1