INFRALAN® LC coupling in metal housing

INFRALAN® LC coupling in metal housing,

The INFRALAN® LC Duplex coupling in metal housing for SC-Simplex breakouts complies with DIN EN 61754-20. Due to the metal housing, it has a higher stability and a low sensitivity to temperature fluctuations. Mounting options include clips or enclosed M2 threaded screws, incl. dust protection caps.

Connector type 1st side: LC Duplex

Connector type 2. side: LC Duplex

Material: metal

Type of mounting: screw/engagement

Sleeve material: Ceramic

Design: SC-Simplex

Operating temperature: -40 to 85°C

Storage temperature: -40 to 85°C

Dimensions: hxbxt 9,3x22x29,2mm

Make: INFRALAN®

Item no.: IKL-LCDU-M-SI